ALS1#show run

Building configuration...

Current configuration : 3143 bytes

!

! Last configuration change at 21:40:52 EET Sun Nov 11 2018

!

version 15.1

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

service compress-config

!

hostname ALS1

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

clock timezone EET 2 0

!

ip cef

!

!

no ip domain-lookup

no ipv6 cef

ipv6 multicast rpf use-bgp

spanning-tree mode pvst

spanning-tree extend system-id

!

!

!

!

!

!

vlan internal allocation policy ascending

!

!

!

!

!

interface Port-channel2

switchport

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

!

interface Port-channel6

switchport

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

!

interface Port-channel1

switchport

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

!

interface Ethernet0/0

duplex auto

!

interface Ethernet0/1

duplex auto

!

interface Ethernet0/2

duplex auto

!

interface Ethernet0/3

duplex auto

!

interface Ethernet1/0

duplex auto

!

interface Ethernet1/1

duplex auto

!

interface Ethernet1/2

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

duplex auto

channel-group 2 mode on

!

interface Ethernet1/3

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

duplex auto

channel-group 2 mode on

!

interface Ethernet2/0

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

duplex auto

channel-group 6 mode on

!

interface Ethernet2/1

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

duplex auto

channel-group 6 mode on

!

interface Ethernet2/2

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

duplex auto

channel-group 1 mode on

!

interface Ethernet2/3

switchport trunk encapsulation dot1q

switchport trunk native vlan 222

switchport trunk allowed vlan 66,100,110,120

switchport mode trunk

duplex auto

channel-group 1 mode on

!

interface Vlan66

ip address 10.1.66.2 255.255.255.0

ipv6 address FE80::A1 link-local

ipv6 address 2001:DB8:CAFE:66::A1/64

!

interface Vlan100

ip address 10.1.100.2 255.255.255.0

ipv6 address FE80::A1 link-local

ipv6 address 2001:DB8:CAFE:100::A1/64

!

interface Vlan110

ip address 10.1.110.2 255.255.255.0

ipv6 address FE80::A1 link-local

ipv6 address 2001:DB8:CAFE:110::A1/64

!

interface Vlan120

ip address 10.1.120.2 255.255.255.0

ipv6 address FE80::A1 link-local

ipv6 address 2001:DB8:CAFE:120::A1/64

!

!

!

no ip http server

!

!

!

!

control-plane

!

!

line con 0

logging synchronous

line aux 0

line vty 0 4

!

ntp update-calendar

ntp server 10.15.2.1

end