R4#show run

Building configuration...

Current configuration : 1464 bytes

!

! Last configuration change at 21:43:23 EET Sun Nov 11 2018

! NVRAM config last updated at 22:43:03 EET Sun Nov 11 2018

!

version 15.5

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname R4

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

!

!

!

bsd-client server url https://cloudsso.cisco.com/as/token.oauth2

clock timezone EET 2 0

mmi polling-interval 60

no mmi auto-configure

no mmi pvc

mmi snmp-timeout 180

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

no ip domain lookup

ip cef

ipv6 unicast-routing

ipv6 cef

!

multilink bundle-name authenticated

!

!

!

key chain ripAuth

key 1

key-string cisco123

!

!

!

!

!

cts logging verbose

!

!

!

redundancy

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

interface Ethernet0/0

no ip address

shutdown

!

interface Ethernet0/1

ip address 10.15.9.1 255.255.255.252

ip rip authentication mode md5

ip rip authentication key-chain ripAuth

ipv6 address FE80::4 link-local

ipv6 address 2001:DB8:CAFE:9::1/64

ipv6 enable

ipv6 rip RIPng enable

!

interface Ethernet0/2

no ip address

shutdown

!

interface Ethernet0/3

no ip address

shutdown

!

router rip

version 2

network 10.0.0.0

no auto-summary

!

ip forward-protocol nd

!

!

no ip http server

no ip http secure-server

!

ipv6 router rip RIPng

!

!

!

!

control-plane

!

!

!

!

!

!

!

!

line con 0

logging synchronous

line aux 0

line vty 0 4

login

transport input none

!

ntp update-calendar

ntp server 10.15.2.1

!

end

R4#