R5#show run

Building configuration...

Current configuration : 1751 bytes

!

! Last configuration change at 20:07:41 EET Sun Nov 11 2018

!

version 15.5

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname R5

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

!

!

!

bsd-client server url https://cloudsso.cisco.com/as/token.oauth2

clock timezone EET 2 0

mmi polling-interval 60

no mmi auto-configure

no mmi pvc

mmi snmp-timeout 180

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

no ip domain lookup

ip cef

ipv6 unicast-routing

ipv6 cef

!

multilink bundle-name authenticated

!

!

!

!

!

!

!

cts logging verbose

!

!

!

redundancy

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

interface Loopback1

ip address 203.15.0.1 255.255.255.252

ipv6 address FE80::5 link-local

ipv6 address 2001:DB8:ABCD::1/64

ipv6 address 2001:DB8:CAFE:1::1/64

!

interface Ethernet0/0

ip address 10.15.0.1 255.255.255.252

ipv6 address FE80::5 link-local

ipv6 address 2001:DB8:CAFE::1/64

!

interface Ethernet0/1

no ip address

shutdown

!

interface Ethernet0/2

no ip address

shutdown

!

interface Ethernet0/3

no ip address

shutdown

!

router bgp 15

bgp router-id 5.7.7.7

bgp log-neighbor-changes

neighbor 10.15.0.2 remote-as 15

!

address-family ipv4

network 10.15.0.0 mask 255.255.255.252

network 203.15.0.0 mask 255.255.255.252

neighbor 10.15.0.2 activate

neighbor 10.15.0.2 next-hop-self

exit-address-family

!

address-family ipv6

neighbor 10.15.0.2 activate

exit-address-family

!

ip forward-protocol nd

!

!

no ip http server

no ip http secure-server

ip route 0.0.0.0 0.0.0.0 10.15.0.2

!

ipv6 route ::/0 2001:DB8:CAFE::2

ipv6 route ::/0 2001:DB8:ABCD::2

!

!

!

control-plane

!

!

!

!

!

!

!

!

line con 0

logging synchronous

line aux 0

line vty 0 4

login

transport input none

!

!

end